1. Swapped pins 120-PB5 and 125-PE0

V1.0



V1.1



1. Changed reset circuit, that resets the microcontroller in case of missing MCO clock:

Diagram, schematic

Description automatically generated

1. Changed reset pullup resistor R93 (10k -> 1k) and reset button series resistor (1k->56R):

Diagram, schematic

Description automatically generated 